    SiS IDE Driver Installation For Windows 95 & Windows 98
   =========================================================
1. Please put SiS IDE Drivers diskette in Floppy drive or
   CD-ROM drive.

2. Please run the file "setup.exe" under "Win9x" directory
   in SiS IDE Drivers diskette and follow the instructions
   to install the SiS IDE Windows 95&98 Driver.

Notice:
*    Does SIS IDE driver support for Windows 98 & Windows 95 OSR2 ?
Ans: Yes, but SiS recommand to use Windows 98 & Windows 95 OSr2 
     default PIO/ DMA driver to get more function supported. 


*  Under Windows 95, system will hang when accessing IDE 
   CD-ROM Driver motion happened, such as open "My Computer", 
   CD-ROM Autoplay ...... etc.

   When this situation happened, 
   SiS suggest remove IDE CD-ROM DOS Driver provided by device 
   company.

   IDE CD-ROM DOS Driver Removing Procedure:

   1. Remark or delete "mscdex.exe"  command in c:\autoexec.bat.
   2. Remark or delete IDE CD-ROM DOS Driver in c:\config.sys.

*  In order to access the removable ZIP drive through SiS driver, the fix
   disk  type  in  BIOS  should be set to "NONE".  If  your  BIOS  always
   automatically detects the disk type, try inserting a ZIP media into the
   ZIP drive when your computer is booting.

