     SiS IDE Driver Un-Installation For Windows NT 4.x
    ===================================================
1.  Enter Windows NT 4.0 System.

2.  Double click the "My Computer" icon on the Desktop.

3.  Select "Control Panel" Folder.

4.  Double click the "SCSI Adapters" applet.

5.  Click on the folder tab labeled "Drivers".
    The currently installed SCSI adapter drivers will be listed in the
    Drivers menu.

    The display should list the SiS Master IDE driver,
    "SiS PCI MASTER IDE Miniport DRIVER"

6.  If the "SiS PCI MASTER IDE Miniport DRIVER" driver is listed,
    select it.  Then, select "Remove" to remove the driver.

7.  Select "Add..." to add a new driver.

8.  Select "Standard mass storage controllers" from "Install Driver".

9.  In the SCSI Adapter dialog, select the default ATAPI driver,
    "IDE CD-ROM (ATAPI 1.2)/Dual-channel PCI IDE Controller"
    and click "Ok" to install the driver.

10. Reboot the system in order for the changes to take effect.




